## Level Meters

The Level meters show the RMS level as a coloured bar and a numeric value at the bottom of the meter and the peak value as a red line and a numeric value at the top of the meter. Levels are in dB below Full Scale.

If the signal generator is playing a sine wave the lower panel shows the gain and phase of the measurement input relative to the reference input at the signal generator frequency, this may be useful for checking inter-channel gain and phase if both channels are fed the same signal.

Help Index