A "house curve" is a target response which differs from that defined by the bass management settings of the speakers. For a detailed description see the discussion in the REW forum at www.hometheatershack.com.

#### Defining a House Curve

The house curve is specified by a set of data that defines an offset that is added to the traces generated from the bass management responses for the speaker type defined. The file containing the house curve data is plain text consisting of pairs of frequency and dB offset values separated by spaces, tabs or commas. Interpolation is used between the pairs of values, either linear or logarithmic (default), according to the state of the Use logarithmic interpolation check box. Logarithmic interpolation draws lines between data points which are straight if the frequency axis is logarithmic. The first and last values in the file are used for all frequencies below and above the range of the data respectively.

- Each line of data must have a frequency value (which is in Hz) and an offset value (which is in dB)
- The points can be at arbitrary frequency spacing, but each line must have a higher frequency than the one before and there must be at least 2 freq, offset data pairs
- Only lines which begin with a number are loaded, others are ignored
- In comma-delimited files there must be at least one space after the comma
- Spaces before values are ignored

The house curve would typically be used to define a boost for the subwoofer range, such as that defined by the data points below. These points give a boost that is 6dB at 20Hz, dropping to 0dB at 80Hz and above. The boost remains flat at 6dB below 20Hz and at 0dB above 80Hz.

                House Curve data

                20 6.0
                80 0.0

When a house curve has been loaded the symbol is displayed next to the Target trace value in the EQ panel.