## SPL Meter

The SPL Meter is an integrating, logging sound level meter that displays sound pressure level, equivalent sound level or sound exposure level based on the RMS level of the input channel. It offers A, C and Z weightings, fast or slow exponential filters, a high pass filter to suppress wind noise, and records minimum, maximum and unweighted peak levels.

The meter takes into account both the soundcard and microphone calibration files and corrects its readings accordingly, allowing IEC class 0 performance when used with a calibrated microphone and SPL calibrator. Note that the maximum boost resulting from the calibration files can be limited by a setting in the Analysis Preferences to prevent excessive boosting of the noise floor. Data recorded by the meter can be logged, graphed and saved to a text file.

The meter displays either sound pressure level (SPL), time-average equivalent sound level (Leq) or sound exposure level (LE) according to the selection made on the buttons below the display. The SPL reading is filtered with either a "Fast" (125ms) or "Slow" (1s) time constant, selected via the F/S buttons. For general use the "Slow" setting is best. When the HP button is pressed a high pass filter is applied that eliminates content below approximately 8Hz.

### Meter Weighting

SPL measurements use weighting curves to shape the signal they receive and emphasise those regions that are of interest for certain requirements. The A and C-weighting curves are shown in the figure below.
C-weighting gives the broadest response (apart from the "Flat", "Zero" or "Z" weighting), with -3dB points at 31.5Hz and 8kHz. A-weighting has a much more pronounced low frequency roll-off. It is modelled on the sensitivity of the ear to low level sounds (about 40dB SPL). A-weighting has the same high frequency roll-off shape as C, but the curves do not align at high frequencies because they are adjusted to both have zero gain at 1kHz, which shifts the A-weighting curve up relative to C-weighting.

### Meter Display

The meter display shows the currently selected measure, the level and an overload ("OVER") indicator which is lit if the soundcard input range is exceeded. The OVER indicator can be reset by clicking in the display area or using the Reset All button. When SPL is selected the display shows dB, the selected weighting in brackets (A, C or Z) and either F for Fast or S for Slow. When measuring equivalent sound level it shows LAeq, LCeq or LZeq according to the selected weighting. SEL is displayed when measuring sound exposure level. The time over which the equivalent sound level or sound exposure level figures have been calculated is shown in the Elapsed Time display at the bottom of the meter. Note that equivalent sound level is useful for making measurements of subwoofer levels using your processor or receiver's internal calibration signal, usually difficult due to the large fluctuations of the level. Equivalent sound level displays a result averaged over the time since Reset All was last pressed; simply start the test signal, press Reset All and wait for the reading to stabilise to get a precise level.

The SPL meter window can be resized as required, the main SPL display digits automatically scale to suit the available space. The meter can also be set to full screen.

Below the main row of controls a level meter shows the current soundcard input level in dBFS, the peak is shown by the red bar while the numeric indicator and the coloured bar show the rms level.

Below the soundcard level meter is a MinMax button to display min, max and peak values in the SPL display and a Reset All button to reset the elapsed time, min, max and peak values, equivalent sound level, sound exposure level and the overload indicator. The Calibrate button starts the meter calibration process, whilst the record button turns the meter on or off. When MinMax is selected the values are displayed alongside the main reading.

### Meter Input Selection

The soundcard input channel which is measured is selected in the Soundcard Preferences. Setting the audio input is described in Getting Started.

### Calibrating the SPL Reading

Valid readings are not displayed until SPL Calibration has been carried out. The SPL reading may be calibrated against an external SPL meter or SPL calibrator by pressing the Calibrate button. The text on the button and the SPL meter digits are red if the meter has not been calibrated. If the soundcard input is altered in the REW soundcard preferences, or if the input levels are altered, it will be necessary to re-calibrate the SPL meter reading.

### SPL Data Logging

The Logger button opens the SPL Logger graph window. The record button in the top right corner of the SPL Logger graph starts or stops logging of SPL values. When logging is in progress the SPL meter on/off, calibrate, weighting, filter time constant and high pass filter buttons are disabled. The logger records the SPL (with the currently selected weighting and time constant), the minimum and maximum values, the unweighted and uncalibrated peak value, the equivalent sound level and the sound exposure level. A Save button above the SPL Logger graph allows the data recorded to be saved to a text file using the text delimiter set in the REW File menu, log files can be loaded using the Open button.

### SPL Logger Controls

The control panel for the SPL logger graph has these controls:

If Show times as time of day is selected the time axis shows the time of day of the logged data, otherwise it shows the elapsed time since logging started. Selecting Log to file using date as filename saves logged data to files in the REW logs directory automatically whenever the logger is running (the directory location is shown in the About REW dialog box). Filenames are formatted as SPL-YYYY-MMM-dd.txt, e.g. SPL-2016-Apr-24.txt. If a file for a day already exists a number will be appended, e.g. SPL-2016-Apr-24-1.txt, SPL-2016-Apr-24-2.txt etc. A new file is created if the logging continues past midnight, with the new date. Note that the files can become very large if logging continues for a long period, growing at about 18 kB per minute. If the option to log to files is selected remember to check the REW log directory to remove files you no longer need.

The format of the logged data is shown below, in this example the text delimiter is Tab and the SPL meter was set to Z weighting.

        SPL log data saved by REW V5.15
        Soundcard cal:
        Mic/meter cal: 7000139.txt
        SPL cal offset: 116.523 dB
        High Pass Filter: Off
        Date: 24-Apr-2016 10:59:07
        Start: 1461495547496

        Time[s]	LZS	LZSMin	LZSMax	LZpeak	LZeq	LZE	Time of day
        0.171	50.1	50.0	50.1	63.5	50.2	42.6	10:59:07.171
        0.341	50.5	50.0	50.5	63.5	51.0	46.3	10:59:07.341
        0.512	50.5	50.0	50.7	63.5	50.8	47.9	10:59:07.512
        0.683	50.5	50.0	50.7	64.1	50.8	49.1	10:59:07.683
        0.853	51.4	50.0	51.4	64.6	51.5	50.8	10:59:07.853

Help Index